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User . Instruction.
Features

1 Primary Address

1 All Call Address

5 Group Addresses

4 line 20-character display 

Stores 65 messages

15 LCD contrast levels

Message received time displayed

Receive alert selectable

Unread message indicator

Backlight

Low Battery indication

Auto on/off

Encryption

Menus


Selecting functions

· To select, Press Scroll Dn (or Up) until desired item shows.

· Press Scroll to select

· Press Read/Select to start/finish.

Basic Operations

· Power On/Off

· Read Messages

· Delete Messages

Power On/Off

Set ON (if unit is off)

· Press and hold Scroll Up until YES  NO shows.

· At Power ON? Select YES.

· Press Read/Select button.  

Set OFF

· Select Power OFF?.

· Select YES/No

· Press Read/Select one time.

Read Message


New At receipt the message is displayed.

Press Read/Select to display.

Stored To review stored messages,

· Select Read All?
· Press Read/Select to display messages and time stamps.

Delete Messages

· Select Delete All
· Press Scroll to select YES/NO

· Press Read/Select button.


Advanced Operations

Assign Tables
Auto ON/OFF

Set Alert Mode
Set Contrast

Set Time/Date
Set Keytone

Select Alert Mode

· Select Set Alert Mode.

· Select Beep.

· Select Loud or Soft

· Select Duration

· Select Vibe

· Select Strong or Weak

· Select Pulse Type

· Select Duration

· Select Both.

· Select Strong or Weak

· Select Duration

Set Time/Date

· Select Set Time/Date.
· Press Read/Select 

· Press Scroll to set each time or date segment and press Read/Select to move through the segments.

Auto ON/OFF

· Select Auto On/Off.

· Press Read/Select.

· Select ON/OFF.

Press Read/Select and Scroll to set on off time segment

Set Contrast

· Select Set Contrast.

· Press Read/Select.

· Scroll DN/UP to adjust.

Set Keytone On/Off

· Select Set Keytone.

· Press Read/Select.

· Select On or Off.

· Press Read/Select to set.

***LRS Recommends DURACELL ONLY to be used – the use of other batteries will affect performance, range and warranty***

Encryption

Encryption is an automatic feature  built into the pager designed to meet HIPAA security requirements.  It is keyed by settings and codes on LRS transmitters.  When encryption is used the pager must be programmed from the encrypted transmitter.
Precautions

Keep unit dry

Don’t self repair

Do not overheat in sunlight

Don’t drop

Don’t use cleaning agents

Don’t use sharp objects on screen

FCC

This equipment complies with FCC rules Class B (digital) Part 15.  This device may not cause harmful interference and this device must accept any interference that may cause undesired operation.
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This is the message that you received this time








